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        Rent Ready Guidelines 
We are committed to providing safe, clean, and properly maintained homes to our residents.
To comply with Western Light standards, the following items must be completed before we advertise and rent a property.

· Property is professionally cleaned and free of trash and debris, inside and outside.
· HVAC system to be in good operating condition, with a new filter installed.
· All mechanical elements including appliances operating as designed.
· Caulking in kitchen and bathrooms shall be clean and free of mildew
· Doors and locks are all functioning properly.
· Windows must open, close, and lock properly and window screens are in good condition.
Full Rent-Ready Requirements 
To comply with both internal and state rental housing requirements, every property must meet the list below in order to be fully advertised and be ‘Rent-Ready’.

☐	Professionally Cleaned to “Hotel Room Clean”
☐	Carpet professionally cleaned and looking fresh
☐	All painted surfaces fresh with no mis-match touch-up areas and repainting must be done corner to corner
☐	All bedroom windows must have vertical or mini blinds and window screens
☐	No personal property or items in the unit or on the property. This includes furniture, knickknacks, toiletries, shower curtains, Kleenex boxes, kitchen or bathroom items, soap dispensers, pictures, etc.
☐	No lawn equipment including mowers, tools, etc.
☐	Garage floor swept
☐	No exterior debris

☐	Lawn cut and trimmed
☐	Landscaping fresh and clean
☐	Carbon monoxide detector installed within 15ft of each bedroom. Smoke/CO2 combo units acceptable
☐	Smoke detectors on each floor and bedroom
☐	Any slider doors must have vertical blinds
☐	All light bulbs working
☐	Doors open and close smoothly and doorsteps installed on all doors 
☐	Bathroom caulking must be fresh and free of mildew
☐	All mechanical components work as designed. Includes HVAC, plumbing and electrical systems, kitchen appliances, laundry appliances (if included), sumps pumps, water softeners, swamp coolers, gas fireplaces, water filtration systems, etc. 
☐	Safety railings secure
☐	Wood-burning fireplace(s), if operational, shall be clean of any debris and have a fireplace screen or heat-proof glass doors installed. If non-operational, the fireplace opening on the interior of the home shall be permanently sealed with an aesthetically pleasing material

*This list is not meant to cover each and make-ready required item, but it does list some of the most important and often overlooked.
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